Camera\_auto\_detect = 1

Moved to /boot/firmware/config.txt

[cm5]

Dtoverlay=dwc2, dr\_mode=host

Deleted:

# dtoverlay=arducam-privariety

Dtoverlay=imx708

imx219 on Raspberry pi 4

* Changed config in the old SD card so that it can identify the camera now
* Installed picamera2 package on raspberry pi, CV2 already installed

- Still cannot show pictures “Camera frontend has timed out”

- Cannot connect to internet “Device-Northwestern” (Already Registered)